
[bookmark: _GoBack]ForceWinder Kawasaki VN 2000 Installation Instructions; Please read these instructions BEFORE installing your new ForceWinder. *Use Blue Loctite on all mounting hardware bolts. 
ATTENTION! A factory service manual may be helpful in performing this installation. Do not attempt to perform this installation if you are not confident in your ability to complete all of the steps in the procedure; consult a trained technician. 
Stock Air Cleaner Removal Instructions:
1. Remove the seat and rear-mounting bolt on the fuel tank.
2. Prop up the rear of the tank; a small block of wood works well. 
3. **Steps 1 & 2 May not be needed. Check n see if removal of air cleaner is easy first.
4. Remove your stock air cleaner and spark plug covers.
5. Keep 4 of the oem stock bolts to re-use on the adapter plate that mounts onto the throttle body.
6. Remove the two hoses that are connected to the back of the air box as well as removing the temp sensor.
7. The one hose will connect to the TOP of the adapter and the other to the LOWER side. The temp sensor will come apart and snap into the lower large diameter hole on the adapter. Please note that there maybe two sizes of the poly elbows needed so we are supplying extras.
8. After the adapter is in place use the smaller gasket supplied and insert the ForceWInder Elbow, once all four ¼ x 20’s are on snug up then tighten.
9. Slip ForceWinder Filter over the Elbow and add the clamp to keep it secure.
10. Slip on Pre Filter Sock and be sure to ride with this sock on the keep your filter clean, remove the filter sock and wash with a liq soap then let dry.
11. Possible re-tune may be needed for optimum performance.
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f g holding the stock carburetor top in place against the tension of the slide
> S— spring, carefully remove the four Phillips screws securing it to the carburetor
o =5 Set the screws aside and slowly remove the stock carburetor top allowing
&, 7, 5 the slde spring extend out of the carburetor body. Leave the side spring in
) e place and b careful not to disturb the siide diaphragm.
oo ormal oo
o.e, S+ a oo STEP 10 Using the stock fasteners, carefully install the new Chrome Carburetor Top/
X T Inner Cup. Make sure the side spring i centered in the new top, the slide diaphragm is in
<L ® 7 2 place in the carburetor body, and that the raised boss s n the correct orientation as
4.3, noted in Step 8. See PIC. 4.
STEP 11 Securely attach the 26 Degree Cylinder Brackes to the cylinder heads
using the stock fasteners removed in STEP 5. Tighten the fasteners securing the
26-Degree Cylinder Brackets to the Chrome Carburetor Top/Inner Cup now as well
STEP 12 Loosely mount the Main Support Bracket. Instal the supplied M6 X 1.0 X
30MM Socket Head Cap Screw and the Chromed, Tapered Bolt Cap at the bottom of the
bracket. With the supplicd gasket on the outside of the bracke, start an M5 X .80 X
16MM Hex Head Cap Screw with an M6 Spiit Lock Washer in the lower right alr cleaner
mounting hole. See PIC. 5
STEP 13 Thread one of the supplied 90-Degree Elbows into the threaded hole on the
side of the Carburetor Manifold included in the kit. Put the Carburetor Manifold in place
slipping the slotted mounting hole into position on the fastener you installed in
the previous step. Install M X .8 X 16MIM Hex Head Cap Screws with M5 Spit Lock
Washers n the remaining two mounting holes. Once all fasteners are i place, tighten
them all securely. Connect hose € from Step 5 to the 90-Degree Elbow with the supplied
7/16" Spring Wire Clamp. See PIC. 6.
STEP 14 Remove the backing from the adhesive on the gasket and install onto the end
of the Carburetor Manifold, making sure the holes n the gasket line up with the holes in
the manifold. See PIC. 6
STEP 15 Hold the fixture ring against the end of the manifold and secure it with the
g three 1/4-20 x 5/8" SHCS screws as shown in PIC. 7
o &
STEP 16 Remove the nylon plug in the bottom of the Corsalr Assembly and install
L 290-Degree barbed fitting
STEP 17 Place the Corsair Assembly on the fixture ring and secure using the four
1/4-20 X 1/2" SHCS screws as shown In PIC. 8.
STEP 18 Install the 5/16" hose on the float bowl vent (where hose A was femoved from in

STEP 5) on the side of the carb (shown in PIC. 9) and use one of the 8" cable ties to secure i
cut of the excess cable te.
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